MONTÁŽ MASKY NA TĚLO VENTILÁTORU 
· Umístěte masku tak, aby její výstupky zapadly do drážek těla ventilátoru (horní strana). 
· Spodní část masky nasaďte tak, aby zajišťovací klip zacvakl do masky. 
· Demontáž masky stisknutím zajišťovacího klipu.
MONTAŽ MASKY NA TELO VENTILÁTORA 
· Umiestnite masku tak, aby jej výstupky zapadli do drážok tela ventilátora (horná strana). 
· Spodnú časť masky nasaďte tak, aby poistka na klik zapadla do masky. 
· Demontáž masky vykonajte stlačením poistky na klik.
INSTALLATION OF THE MASK ON THE FAN BODY 
· Position the mask so that its teeth fall into the slofan body (top side). 
· Place the lower part of the mask so that the safety button clicks into place into the mask. 
· Dismantle the mask by pressing the safety button.
[bookmark: _GoBack][image: ]
image1.png
v [B MASKAPOLUOBLA A100M copy ¢ X | B} MASKA POLUOBLA MATSTAKLO / X [ RAM ZA PLOCICE A100M copy PR X |

< O

“

¥ v ¥V Nacrtaj

Q

A

(@ Datoteka C:/Users/andje/AppData/Local/Temp/Rar$DIa0.486/RAM%20ZA%20PLOCICE%20A100M%20copy%20PREVOD. pdf

as | @ Ppitajte Copilot v - 4+ 2 oda | @) | (B

MONTAZ MASKY NA TELO VENTILATORA

- Umiestnite masku tak, aby jej vystupky zapadli do dréZok tela ventilatora (horna strana).
- Spodnu ¢ast masky nasadte tak, aby poistka na klik zapadla do masky.

- Demontaz masky vykonajte stlaéenim poistky na klik.

INSTALLATION OF THE MASK ON THE FAN BODY

-Position the mask so that its teeth fall into the slotfan body (top side).

-Place the lower part of the mask so that the fuse clicks into place into the mask.
-Dismantle the mask by pressing the safety button.
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